**Description of this EMUNE code:**

**Including:**

This package includes the EMUNE source codes, main input file and test files. (the output file of current problem described in the main input is also included)

**Main input file:**

The name of node and element files written in the main input file; also the input parameters are included in the main input file (iteration number, material properties, Horizon, initial crack, damage index)

**Problem description:**

In this code, the sudden load is applied at the top and bottom boundary (in the module of dynamics). The precrack is introduced in the main input file.